*Heading
** Job name: eckegrob Model name: Model-1
** Generated by: Abaqus/CAE 6.12-3
*Preprint, echo=NO, model=NO, history=NO, contact=NO
*Node, NSET=ALL
**
** UEL elements (material included in implementation) **
**
*USER ELEMENT,NODES=4,TYPE=U1003,PROPERTIES=1,COORDINATES=3,VARIABLES=1
*ELEMENT,TYPE=U1003,ELSET=UELS
*UEL PROPERTY,ELSET=UELS
*Nset, nset=Set-5
*Nset, nset=Set-6
** ----------------------------------------------------------------
**
** STEP: Step-1
**
*Step, name=Step-1, nlgeom=YES
*Static
1.0,1.0,1e-05,1.0
**Solution Technique, TYPE=QUASI-NEWTON
*Controls, ANALYSIS=DISCONTINUOUS
**
** BOUNDARY CONDITIONS
**
** Name: BC-1 Type: Displacement/Rotation
*Boundary
6,1,1
6,2,2
6,3,3
3,3,3
*Boundary
**Set-5, 1, 1
Set-5, 2, 2
**Set-5, 3, 3
** Name: BC-2 Type: Displacement/Rotation
*Boundary
**Set-6, 1, 1
Set-6, 2, 2, 0.1
**Set-6, 3, 3
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field, frequency=1
*Node Output
U, RF, NT
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step